{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":20,"n_cols":5,"rows_kept":20,"merged":[[0,0,0,5],[2,4,2,5],[3,4,3,5],[4,4,4,5],[5,4,5,5],[6,4,6,5],[7,4,7,5],[8,4,8,5],[9,4,9,5],[10,4,10,5],[11,4,11,5],[13,4,13,5],[14,4,14,5],[15,4,15,5],[16,4,16,5],[17,4,17,5],[18,4,18,5],[19,0,19,5]],"flags":["formulas_cached_only"]}
["录音棚装修明细"]
["一、 ","声学装修部分"]
["序号","项目名称","单位","数量","技术参数"]
[1,"钢制成品隔声门(单开)","套",2,"隔声量≥30dB,2000mm高×900mm宽×60mm厚"]
[2,"隔声门窗包套","套",4,"基层木工板，9mm纤维吸音面板，阻燃B1级，环保E1级。"]
[3,"墙顶面木龙骨结构9厚纤维吸音板面层","m2",140,"9mm纤维吸音板，阻燃B1级，环保E1级。"]
[4,"木质踢脚线","m",35,"60mm成品踢脚线，强化复合踢脚线"]
[5,"地铺复合地板","m2",40,"阻燃B1级，环保E1级。"]
[6,"钢化玻璃隔音观察窗","项",1,"三层非平行结构"]
[7,"隔音通风窗","项",2,"双层结构，外层隔音玻璃，内层隔声吸音结构"]
[8,"      墙顶面1200mmX600mmX50mm多频段声学模块调音板","块 ",28,"采用多层材料进行声学处理，外表穿孔面板除声学作用外还具备高端的装饰效果，边框采用带线条铝合金，整体美观可拆卸减震安装方式。降噪系数NRC=0.85,吸声构造的吸声性能为1级。（具备实用新型专利证书）"]
[9,"      顶面600mmX600mmX50mm单频段声学模块调音板","块 ",10,"采用多层材料进行声学处理，外表穿孔面板除声学作用外还具备高端的装饰效果，边框采用带线条铝合金，整体美观可拆卸减震安装方式。降噪系数NRC=0.85,吸声构造的吸声性能为1级。（具备实用新型专利证书）"]
["二、 ","其他装修部分"]
[1,"杂物拆除垃圾清运费","项",1,"施工垃圾装袋由工地清运到室外建筑垃圾堆放点"]
[2,"材料二次搬运","项",1,"施工材料由室外搬运到室内工地"]
[3,"LED射灯、筒灯","套",26,"LED灯6W亮度。"]
[4,"开关、插座","个",20,"单相暗插座安装 10A 5孔，单开面板、双开面板。插座面板20个、单开面板3个、双开面板3个"]
[5,"灯具安装费","项",1,"日光灯具安装 成套型 吸顶式 筒灯，安装费不计取未计价材料费用"]
[6,"强电路改造","m2  ",38,"动力线路管内穿铜芯导线 ，20镀锌贴管，设备配线规格4m2 3线组合铜电线100米、照明配线规格2.5m2，3线组合铜电线100米；配管嵌入式暗装结构，但无需墙体剔槽装入吸音层结构。"]
["    本案为录音棚设计搭建，套内面积约44平米，包括：声学设计、隔音门窗处理隔声量≥45dB，吸音材料等工作,降噪系数NRC=0.80,吸声构造的吸声性能为1级。 吸音材料达到国家B1级防火标准,国家E1级环保标准 ."]