{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"merged":[[0,0,0,5],[37,0,37,5]],"flags":["formulas_cached_only"]}
["附件2：LX2019-014(分包2）项目需求"]
["A","音响系统"]
["序号","名称","品牌型号","技术指标","数量","单位"]
[1,"线阵列全频","ZSOUND－LA110","频率响应:60Hz－18KHz             阻抗:HF/LF 16/16ohm          功率:HF/LF 80W/350W                 ",12,"只"]
[2,"线阵列低音","ZSOUND－LA110S","频率响应:40HZ－200HZ             阻抗:8ohm       功率:1000W",4,"只"]
[3,"舞台监听","ZSOUND－M15","频率响应:50HZ－18KHZ             阻抗:8ohm        功率:450W",4,"只"]
[4,"处理器","ZSOUND－M44T","4进4出数字处理器",2]
[5,"功放","ZSOUND－M1300Q","四通道专业功放频率响应:20HZ－25KHZ电源要求:200－240V",4,"台"]
[6,"电源","TCD－4","4＊WP6 16A3P 信号电源分配盒",2,"台"]
[7,"调音台","mdias－M32","32路输入通道，16个AUX输出，6个编组，LCR主输出   支持AES50网络，可 ipad 和 iphone 遥控控制        16种效果器",1,"台"]
[8,"麦克风","无线手持","SHURE（舒尔） SM8 心型和超心型指向",6,"只"]
[9,"音响线",null,"配套",1,"批"]
[10,"电源线",null,"配套",1,"批"]
[11,"信号线",null,"配套",1,"批"]
[12,"话筒架",null,"配套",1,"批"]
["B","灯光系统",null,null,"数量","单位"]
[1,"MA","Z6","灯光控台 主台一张，备份台一张",1,"台"]
[2,"追光灯","筑梦1700R","用于演员特型面光，如主持",2,"台"]
[3,"电脑摇头光束灯","DENL330三合一","用于全场光束效果，顶光4道",48,"台"]
[4,"电脑摇头光束灯","DENL330三合一","用于全场光束效果，地面逆光一道",16,"台"]
[5,"摇头变焦LED","ZM-12","用于舞台染色  顶部逆光光2道",32,"台"]
[6,"烟雾机","KS-500","用于渲染舞台光束效果",2,"台"]
[7,"面光切割灯","筑梦1400","用于舞台面光，",5,"只"]
[8,"切割灯","筑梦1400","用于舞台定点光 顶部5道吊杆",25,"台"]
[9,"led顶光","SL354","用于舞台染色 顶光4道",48,"只"]
[10,"电脑染色灯","筑梦1400","用于舞台侧光，每侧高低流各8台",16,"台"]
[11,"硅群","12*6000W","用于常规灯及电脑灯等设备电路连接",1,"组"]
[12,"配套弱电连接线",null,"信号线，分配器，放大器等",1,"批"]
[13,"配套强电连接线",null,"25平方电缆线  2.5平方连接线",1,"批"]
[14,"其它必要的配件",null,"灯泡，烟油，等耗材",1,"批"]
[15,"灯光师劳务","    ","专业演出灯光师",1,"场"]
["C","视频系统",null,null,"数量","单位"]
[1,"LED高清大屏幕","P3","舞台侧面节目提示屏",6,"平方"]
[2,"视频服务器",null,"切换",1,"台"]
["D","运费及人工",null,null,"数量","单位"]
[1,"运费","根据实际公里数","设备运输",6,"车/次"]
[2,"人工",null,"1天安装，2天走台合光，2天演出",24,"人/次"]
["注：清单中品牌型号为推荐品牌型号，供应商所投租赁的产品的技术参数需相当或优于推荐品牌型号，否则响应文件无效。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}